;****************************************************************
; ASIX AX88772B USB2.0 to Fast Ethernet Adapter
;
; Copyright 2010, ASIX Electronics Corporation
;
; Version: 5.12.3.0	for windows 7 32-bit
;****************************************************************
[Version]
Signature  = "$Windows NT$"
CatalogFile = ax88772bex.cat
Class      = Net
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider   = %ASIX%
DriverVer = 05/21/2010, 5.12.3.0

[Manufacturer]
%ASIX%   = USB, NTx86.6.1

[ControlFlags]
ExcludeFromSelect = USB\VID_0B95&PID_772B

[USB.NTx86.6.1]
%AX88772B.DeviceDesc% = AX88772B.Ndi,USB\VID_0B95&PID_772B

;****************************************************************
[AX88772B.Ndi]
AddReg          = AX88772B.NT.Reg, AX88772B.Con.Reg
Characteristics = 0x84
BusType         = 15
CopyFiles       = CopyFile.Sys
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[AX88772B.Ndi.Services]
AddService = AX88772B, 2, AX88772B.Service, Common.EventLog

[AX88772B.Ndi.WMI]
WMIInterface={7F90DE09-B457-41b4-B9DA-604C550FB6C1},,WMIGuidSecurity_AllReadAdminFul
WMIInterface={7F90DE09-B457-41b4-B9DA-604C550FB6C2},,WMIGuidSecurity_AllReadAdminFul
WMIInterface={7F90DE09-B457-41b4-B9DA-604C550FB6C3},,WMIGuidSecurity_AllReadAdminFul

[WMIGuidSecurity_AllReadAdminFul]
security="O:BAG:BAD:(A;;0x12001f;;;BA)(A;;0x12001f;;;LS)(A;;0x12001f;;;NS)(A;;0x12001f;;;SY)(A;;0x12001f;;;NO)(A;;CC;;;BU)"

;****************************************************************
; Driver parameters
;****************************************************************
[AX88772B.Con.Reg]
HKR, ,               ChipCode,   0, "2"

; Connection Type
HKR,Ndi\params\*SpeedDuplex,ParamDesc,,%ConnectionType%
HKR,Ndi\params\*SpeedDuplex,default,,"0"
HKR,Ndi\params\*SpeedDuplex,type,,"enum"
HKR,Ndi\params\*SpeedDuplex\enum,0,,%AutoSense%
HKR,Ndi\params\*SpeedDuplex\enum,1,,%10Half%
HKR,Ndi\params\*SpeedDuplex\enum,2,,%10Full%
HKR,Ndi\params\*SpeedDuplex\enum,3,,%100Half%
HKR,Ndi\params\*SpeedDuplex\enum,4,,%100Full%

; Mac Address
HKR,Ndi\params\NetworkAddress,ParamDesc,0,%NetworkAddress%
HKR,Ndi\params\NetworkAddress,type,0,"edit"
HKR,Ndi\params\NetworkAddress,default,0, "000000000000"
HKR,Ndi\params\NetworkAddress,LimitText,0,"12"
HKR,Ndi\params\NetworkAddress,UpperCase,0,"1"
HKR,Ndi\params\NetworkAddress,Optional,0,"1"

; Flow Control
HKR,Ndi\params\*FlowControl,ParamDesc,,%FlowControl%
HKR,Ndi\params\*FlowControl,default,,"3"
HKR,Ndi\params\*FlowControl,type,,"enum"
HKR,Ndi\params\*FlowControl\enum,0,,%Disabled%
HKR,Ndi\params\*FlowControl\enum,1,,%TxEnabled%
HKR,Ndi\params\*FlowControl\enum,2,,%RxEnabled%
HKR,Ndi\params\*FlowControl\enum,3,,%TxRxEnabled%

; Wake Up
HKR,Ndi\params\WakeUp,ParamDesc,,%WakeUp%
HKR,Ndi\params\WakeUp,default,,"0"
HKR,Ndi\params\WakeUp,type,,"enum"
HKR,Ndi\params\WakeUp\enum,0,,%Disabled%
HKR,Ndi\params\WakeUp\enum,2,,%LinkChange%
HKR,Ndi\params\WakeUp\enum,4,,%MagicPacket%
HKR,Ndi\params\WakeUp\enum,8,,%WakeUpFrame%
HKR,Ndi\params\WakeUp\enum,6,,%LinkChange-MagicPacket%
HKR,Ndi\params\WakeUp\enum,10,,%LinkChange-WakeUpFrame%
HKR,Ndi\params\WakeUp\enum,12,,%MagicPacket-WakeUpFrame%
HKR,Ndi\params\WakeUp\enum,14,,%All%

;Wake Up Frame
HKR,Ndi\params\WakeUpFrameType,ParamDesc,,%WakeUpFrameType%
HKR,Ndi\params\WakeUpFrameType,default,,"0"
HKR,Ndi\params\WakeUpFrameType,type,,"enum"
HKR,Ndi\params\WakeUpFrameType\enum,0,,%WindowsDefault%
HKR,Ndi\params\WakeUpFrameType\enum,1,,%PING%
HKR,Ndi\params\WakeUpFrameType\enum,2,,%ARP%
HKR,Ndi\params\WakeUpFrameType\enum,3,,%PING-ARP%

; Qos Packet Tagging
HKR,Ndi\params\QosTag,ParamDesc,,%QoSTagging%
HKR,Ndi\params\QosTag,default,,"0"
HKR,Ndi\params\QosTag,type,,"enum"
HKR,Ndi\params\QosTag\enum,0,,%Disabled%
HKR,Ndi\params\QosTag\enum,1,,%Enabled%

;VLAN ID
HKR, Ndi\Params\VLAN_ID,  ParamDesc,  , %VLANID%
HKR, Ndi\Params\VLAN_ID,  Type,       , "int"
HKR, Ndi\Params\VLAN_ID,  Default,    , "0"
HKR, Ndi\params\VLAN_ID,  min,        , "0"
HKR, Ndi\params\VLAN_ID,  max,        , "4095"
HKR, Ndi\params\VLAN_ID,  step,       , "1"
HKR, NDI\params\VLAN_ID,  UpperCase,  , "1"
HKR, NDI\params\VLAN_ID,  optional,   , "1"

; TCP Checksum offload V4
HKR, Ndi\params\*TCPChecksumOffloadIPv4,ParamDesc,0,"%TCPChecksumOffloadV4%"	
HKR, Ndi\params\*TCPChecksumOffloadIPv4,default,0,"3"
HKR, Ndi\params\*TCPChecksumOffloadIPv4,type,0,"enum"
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,"0",0,"%Disabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,"1",0,"%TxEnabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,"2",0,"%RxEnabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,"3",0,"%TxRxEnabled%"

; UDP Checksum offload V4
HKR, Ndi\params\*UDPChecksumOffloadIPv4,ParamDesc,0,"%UDPChecksumOffloadV4%"	
HKR, Ndi\params\*UDPChecksumOffloadIPv4,default,0,"3"
HKR, Ndi\params\*UDPChecksumOffloadIPv4,type,0,"enum"
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,"0",0,"%Disabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,"1",0,"%TxEnabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,"2",0,"%RxEnabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,"3",0,"%TxRxEnabled%"

; TCP Checksum offload V6
HKR, Ndi\params\*TCPChecksumOffloadIPv6,ParamDesc,0,"%TCPChecksumOffloadV6%"	
HKR, Ndi\params\*TCPChecksumOffloadIPv6,default,0,"3"
HKR, Ndi\params\*TCPChecksumOffloadIPv6,type,0,"enum"
HKR, Ndi\params\*TCPChecksumOffloadIPv6\enum,"0",0,"%Disabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv6\enum,"1",0,"%TxEnabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv6\enum,"2",0,"%RxEnabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv6\enum,"3",0,"%TxRxEnabled%"

; UDP Checksum offload V6
HKR, Ndi\params\*UDPChecksumOffloadIPv6,ParamDesc,0,"%UDPChecksumOffloadV6%"	
HKR, Ndi\params\*UDPChecksumOffloadIPv6,default,0,"3"
HKR, Ndi\params\*UDPChecksumOffloadIPv6,type,0,"enum"
HKR, Ndi\params\*UDPChecksumOffloadIPv6\enum,"0",0,"%Disabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv6\enum,"1",0,"%TxEnabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv6\enum,"2",0,"%RxEnabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv6\enum,"3",0,"%TxRxEnabled%"

; IP Checksum offload V4
HKR, Ndi\params\*IPChecksumOffloadIPv4,ParamDesc,0,"%IPChecksumOffloadV4%" 
HKR, Ndi\params\*IPChecksumOffloadIPv4,default,0,"3"
HKR, Ndi\params\*IPChecksumOffloadIPv4,type,0,"enum"
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,"0",0,"%Disabled%"
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,"1",0,"%TxEnabled%"
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,"2",0,"%RxEnabled%"
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,"3",0,"%TxRxEnabled%"

; ARP offload
HKR,Ndi\params\*PMARPOffload,ParamDesc,,%ArpOffload%
HKR,Ndi\params\*PMARPOffload,default,,"0"
HKR,Ndi\params\*PMARPOffload,type,,"enum"
HKR,Ndi\params\*PMARPOffload\enum,0,,%Disabled%
HKR,Ndi\params\*PMARPOffload\enum,1,,%Enabled%

; NS offload
HKR,Ndi\params\*PMNSOffload,ParamDesc,,%NsOffload%
HKR,Ndi\params\*PMNSOffload,default,,"0"
HKR,Ndi\params\*PMNSOffload,type,,"enum"
HKR,Ndi\params\*PMNSOffload\enum,0,,%Disabled%
HKR,Ndi\params\*PMNSOffload\enum,1,,%Enabled%

; AutoDetach
HKR, Ndi\params\AutoDetach,ParamDesc,0,"%AutoDetach%" 
HKR, Ndi\params\AutoDetach,default,0,"2"
HKR, Ndi\params\AutoDetach,type,0,"enum"
HKR, Ndi\params\AutoDetach\enum,"0",0,"%Disabled%"
HKR, Ndi\params\AutoDetach\enum,"1",0,"%Enabled%"
HKR, Ndi\params\AutoDetach\enum,"2",0,"%UseEeprom%"

; WOL Link Speed
HKR, Ndi\params\WolLinkSpeed,ParamDesc,0,"%WolLinkSpeed%" 
HKR, Ndi\params\WolLinkSpeed,default,0,"1"
HKR, Ndi\params\WolLinkSpeed,type,0,"enum"
HKR, Ndi\params\WolLinkSpeed\enum,"0",0,"%10mFirst%"
HKR, Ndi\params\WolLinkSpeed\enum,"1",0,"%UseEeprom%"

; Mask WakeUp Event Timer
HKR, Ndi\params\MaskTimer,ParamDesc,0,"%MaskTimer%" 
HKR, Ndi\Params\MaskTimer,default,0,"1"
HKR, Ndi\Params\MaskTimer,type,0,"enum"
HKR, Ndi\params\MaskTimer\enum,"0",0,"%0sec%"
HKR, Ndi\params\MaskTimer\enum,"1",0,"%4sec%"
HKR, Ndi\params\MaskTimer\enum,"2",0,"%8sec%"
HKR, Ndi\params\MaskTimer\enum,"3",0,"%12sec%"
HKR, Ndi\params\MaskTimer\enum,"4",0,"%16sec%"
HKR, Ndi\params\MaskTimer\enum,"5",0,"%20sec%"
HKR, Ndi\params\MaskTimer\enum,"6",0,"%24sec%"
HKR, Ndi\params\MaskTimer\enum,"7",0,"%28sec%"

;****************************************************************
; Install section for Windows NT 5
;****************************************************************
[AX88772B.NT.Reg]
; Interfaces
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi,            Service,    0, "AX88772B"

HKR,,LogErrorMessages, 0, "1"

[AX88772B.Service]
DisplayName    = %AX88772B.DeviceDesc%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\ax88772b.sys
LoadOrderGroup = NDIS

[Common.EventLog]
AddReg = Common.AddEventLog.Reg

[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\system32\drivers\ax88772b.sys"
HKR, , TypesSupported  , 0x00010001, 7

[CopyFile.Sys]
ax88772b.sys,,,2

;****************************************************************
; WDF Coinstaller installation section
;****************************************************************
[AX88772B.Ndi.CoInstallers]
AddReg=AX88772B.CoInstaller.AddReg
CopyFiles=AX88772B.CoInstaller.CopyFiles

[AX88772B.CoInstaller.AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01009.dll,WdfCoInstaller"

[AX88772B.CoInstaller.CopyFiles]
WdfCoInstaller01009.dll

[AX88772B.Ndi.Wdf]
KmdfService = AX88772B, AX88772B.wdfsect

[AX88772B.wdfsect]
KmdfLibraryVersion = 1.9

;**********************************************************************
; Destination directories
;**********************************************************************
[DestinationDirs]
CopyFile.Sys	= 12
AX88772B.CoInstaller.CopyFiles = 11

[SourceDisksNames]
1=%AX88772B.DiskName%,,

[SourceDisksFiles]
ax88772b.sys=1,,ax88772b.sys,10000
WdfCoInstaller01009.dll = 1

;**********************************************************************
; Localizable strings
;**********************************************************************
[Strings]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

;Chinese_Taiwan
[Strings.0404]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "連線速度"
AutoSense              = "自動偵測"
10Half                 = "10BaseT 半雙工"
10Full                 = "10BaseT 全雙工"
100Half                = "100BaseTx 半雙工"
100Full                = "100BaseTx 全雙工"
NetworkAddress         = "網路卡位址"
FlowControl            = "流量控制"
Disabled               = "關閉"
Enabled                = "開啟"
TxEnabled              = "Tx 開啟"
RxEnabled              = "Rx 開啟"
TxRxEnabled            = "Rx & Tx 開啟"
WakeUp                 = "網路喚醒"
LinkUp                 = "網路連接"
MagicPacket            = "魔術封包"
WakeUpFrame            = "喚醒封包"
LinkUp-MagicPacket     = "網路連接/魔術封包"
LinkUp-WakeUpFrame     = "網路連接/喚醒封包"
MagicPacket-WakeUpFrame= "魔術封包/喚醒封包"
LinkChange             = "網路更改"
LinkChange-MagicPacket = "網路更改/魔術封包"
LinkChange-WakeUpFrame = "網路更改/喚醒封包"
All                    = "全部"
Both                   = "兩者"
QoSTagging             = "QoS封包標籤"
WakeUpFrameType        = "喚醒封包類型"
WindowsDefault         = "Windows 內定"
PING                   = "PING封包"
ARP                    = "ARP封包"
PING-ARP               = "PING封包/ARP封包"
VLANID                 = "虛擬區域網路編號"
TCPChecksumOffloadV4   = "TCP 檢查總和卸載 (IPv4)"
UDPChecksumOffloadV4   = "UDP 檢查總和卸載 (IPv4)"
TCPChecksumOffloadV6   = "TCP 檢查總和卸載 (IPv6)"
UDPChecksumOffloadV6   = "UDP 檢查總和卸載 (IPv6)"
IPChecksumOffloadV4    = "IPv4 檢查總和值卸載"
AutoDetach             = "AutoDetach"
UseEeprom              = "使用EEPROM設定"
WolLinkSpeed           = "WOL 連線速度"
10mFirst               = "10 Mbps 優先"
MaskTimer              = "遮蔽喚醒事件計時器"
0sec                   = "0 秒"
4sec                   = "4 秒"
8sec                   = "8 秒"
12sec                  = "12 秒"
16sec                  = "16 秒"
20sec                  = "20 秒"
24sec                  = "24 秒"
28sec                  = "28 秒"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

;Chinese_PRC
[Strings.0804]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "链接类型"
AutoSense              = "自动检测"
10Half                 = "10BaseT 半双工"
10Full                 = "10BaseT 全双工"
100Half                = "100BaseTx 半双工"
100Full                = "100BaseTx 全双工"
NetworkAddress         = "网络地址"
FlowControl            = "流量控制"
Disabled               = "禁用"
Enabled                = "启用"
TxEnabled              = "Tx 启用"
RxEnabled              = "Rx 启用"
TxRxEnabled            = "Rx & Tx 启用"
WakeUp                 = "唤醒"
LinkUp                 = "链接建立"
MagicPacket            = "魔术包"
WakeUpFrame            = "唤醒帧"
LinkUp-MagicPacket     = "链接建立/魔术包"
LinkUp-WakeUpFrame     = "链接建立/唤醒帧"
MagicPacket-WakeUpFrame= "魔术包/唤醒帧"
LinkChange             = "链接更改"
LinkChange-MagicPacket = "链接更改/魔术包"
LinkChange-WakeUpFrame = "链接更改/唤醒帧"
All                    = "全部"
Both                   = "两者"
QoSTagging             = "Qos封包标签"
WakeUpFrameType        = "唤醒帧类型"
WindowsDefault         = "Windows 缺省"
PING                   = "PING包"
ARP                    = "ARP包"
PING-ARP               = "PING包/ARP包"
VLANID                 = "VLAN标识"
TCPChecksumOffloadV4   = "TCP校验和承载(IPv4)"
UDPChecksumOffloadV4   = "UDP校验和承载(IPv4)"
TCPChecksumOffloadV6   = "TCP校验和承载(IPv4)"
UDPChecksumOffloadV6   = "UDP校验和承载(IPv6)"
IPChecksumOffloadV4    = "IPv4校验和承载"
AutoDetach             = "AutoDetach"
UseEeprom              = "采用EEPROM设置"
WolLinkSpeed           = "WOL链接速率"
10mFirst               = "10 Mbps 优先"
MaskTimer              = "屏蔽唤醒事件定时器"
0sec                   = "0 秒"
4sec                   = "4 秒"
8sec                   = "8 秒"
12sec                  = "12 秒"
16sec                  = "16 秒"
20sec                  = "20 秒"
24sec                  = "24 秒"
28sec                  = "28 秒"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

;Japaness
[Strings.0411]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "接続タイプ"
AutoSense              = "自動認識"
10Half                 = "10BaseT 半二重"
10Full                 = "10BaseT 全二重"
100Half                = "100BaseTx 半二重"
100Full                = "100BaseTx 全二重"
NetworkAddress         = "ネットワークアドレス"
FlowControl            = "帯域制御"
Disabled               = "不可"
Enabled                = "可"
TxEnabled              = "Tx 使用可(On)"
RxEnabled              = "Rx 使用可(On)"
TxRxEnabled            = "Rx & Tx 使用可(On)"
WakeUp                 = "ウェイクアップ"
LinkUp                 = "リンクアップ"
MagicPacket            = "マジック・パケット"
WakeUpFrame            = "ウェイクアップ・フレーム"
LinkUp-MagicPacket     = "リンクアップ/マジック・パケット"
LinkUp-WakeUpFrame     = "リンクアップ/ウェイクアップ・フレーム"
MagicPacket-WakeUpFrame= "マジック・パケット/ウェイクアップ・フレーム"
LinkChange             = "リンクチェンジ"
LinkChange-MagicPacket = "リンクチェンジ/マジック・パケット"
LinkChange-WakeUpFrame = "リンクチェンジ/ウェイクアップ・フレーム"
All                    = "全て"
Both                   = "両方"
QoSTagging             = "QoSパケット・タグ"
WakeUpFrameType        = "ウェイクアップフレーム・タイプ"
WindowsDefault         = "Winodwsデフォルト"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCPチェックサム・オフロード(IPv4)"
UDPChecksumOffloadV4   = "UDPチェックサム・オフロード(IPv4)"
TCPChecksumOffloadV6   = "TCPチェックサム・オフロード(IPv6)"
UDPChecksumOffloadV6   = "UDPチェックサム・オフロード(IPv6)"
IPChecksumOffloadV4    = "IPv4 チェックサム・オフロード"
AutoDetach             = "AutoDetach"
UseEeprom              = "使用EEPROMの設定"
WolLinkSpeed           = "WOLリンクスピード"
10mFirst               = "10Mbps 優先"
MaskTimer              = "ウェイクアップ事象タイマ・マスク"
0sec                   = "0 秒"
4sec                   = "4 秒"
8sec                   = "8 秒"
12sec                  = "12 秒"
16sec                  = "16 秒"
20sec                  = "20 秒"
24sec                  = "24 秒"
28sec                  = "28 秒"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

;Korean
[Strings.0412]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "접속형태"
AutoSense              = "자동감지"
10Half                 = "10BaseT 반이중"
10Full                 = "10BaseT 전이중"
100Half                = "100BaseTx 반이중"
100Full                = "100BaseTx 전이중"
NetworkAddress         = "네트웍 주소"
FlowControl            = "플로우 제어"
Disabled               = "해제"
Enabled                = "설정"
TxEnabled              = "Tx 설정"
RxEnabled              = "Rx 설정"
TxRxEnabled            = "Rx & Tx 설정"
WakeUp                 = "웨이크업"
LinkUp                 = "링크업"
MagicPacket            = "매직패킷"
WakeUpFrame            = "웨이크업 프레임"
LinkUp-MagicPacket     = "링크업/매직패킷"
LinkUp-WakeUpFrame     = "링크업/웨이크업 프레임"
MagicPacket-WakeUpFrame= "매직패킷/웨이크업 프레임"
LinkChange             = "링크변경"
LinkChange-MagicPacket = "링크변경/매직패킷"
LinkChange-WakeUpFrame = "링크변경/웨이크업 프레임"
All                    = "전체"
Both                   = "양측"
QoSTagging             = "QoS 패킷 태깅"
WakeUpFrameType        = "웨이크업 프레임 형태"
WindowsDefault         = "윈도우 기본값"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN 아이디"
TCPChecksumOffloadV4   = "TCP 첵섬 오프로드(IPv4)"
UDPChecksumOffloadV4   = "UDP 첵섬 오프로드(IPv4)"
TCPChecksumOffloadV6   = "TCP 첵섬 오프로드(IPv6)"
UDPChecksumOffloadV6   = "UDP 첵섬 오프로드(IPv6)"
IPChecksumOffloadV4    = "IPv4 첵섬 오프로드"
AutoDetach             = "AutoDetach"
UseEeprom              = "EEPROM이 설정을 사용"
WolLinkSpeed           = "WoL 연결 속도"
10mFirst               = "10Mbps 우선"
MaskTimer              = "웨이크업 이벤트 타이머 차단"
0sec                   = "0 초"
4sec                   = "4 초"
8sec                   = "8 초"
12sec                  = "12 초"
16sec                  = "16 초"
20sec                  = "20 초"
24sec                  = "24 초"
28sec                  = "28 초"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

;Germany
[Strings.0407]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Verbindungstyp"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "Netzwerkadresse"
FlowControl            = "Flow Control"
Disabled               = "Ausgeschaltet"
Enabled                = "Eingeschaltet"
TxEnabled              = "Tx Eingeschaltet"
RxEnabled              = "Rx Eingeschaltet"
TxRxEnabled            = "Rx & Tx Eingeschaltet"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "Alles"
Both                   = "Beides"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.0406]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.0408]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.040a]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.040b]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.040c]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.040d]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.040e]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.0410]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.0413]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.0414]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.0415]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.0416]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.0419]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.041d]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.041e]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.041f]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.0424]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.042a]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"

[Strings.3801]
ASIX = "ASIX"
AX88772B.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772B.DeviceDesc = "ASIX AX88772B USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
LinkChange             = "Link Change"
LinkChange-MagicPacket = "Link Change/Magic Packet"
LinkChange-WakeUpFrame = "Link Change/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"
